|  |
| --- |
| Use Case: *Handover Control* |
| ID: *3* |
| Goal: *ATCC handovers control to APC* |
| Primary actor: *ATCC* |
| Secondary actor(s): *Pilot* |
| Preconditions:   1. *An aircraft approaches the control zone* |
| Post-conditions:   1. *APC takes control of the aircraft.* 2. *Pilot contacts the APC* |
| Main flow:   1. *ATCC controller sends EFPS and alerts APC about the aircraft* 2. *EFPS is set as pending* 3. *APC receives the EFPS and sends a confirmation to ATCC* 4. *ATCC controller instructs the pilot to contact APC* 5. *Pilot receives the instruction* |
| Alternative flows:  *3a. ATCC does not receive confirmation.*   1. *Repeat step 1 in the main flow* 2. *Return to step 3* |